Kalman Filters don’t need to only be used with sequential measurements from one sensor. It can be used to combine measurements from different sensors.

We can use LIDAR and RADAR sensors together to overcome each of their individual weaknesses to estimate things like pedestrian location, heading, and speed.

